
**FRESH-AIRE UV COMMERCIAL SIZING SURVEY**

Fresh-Aire UV has two HVAC disinfection options. Learn more below.

**Option A)** coil/air handler disinfection, which is ideal for maintaining a clean coil, drain pan and surfaces within the AHU addressing any biological blow-off and all-around air treatment. You would provide the size of the coil. Fresh-Aire UV also offers systems for high-level air disinfection **option B)** which are parallel lamp systems that are mounted in the return or supply that provides a higher level of airstream disinfection. These are typically used in healthcare applications such as operating and patient rooms.

If you are looking for airstream disinfection we can size the lamp systems for the coil/air handler (option A) and can “oversize” so we can also address the moving air better, or should you wish, please provide the duct dimensions (return or supply) and CFM and we can base our sizing calculations on our ADS system (option B). Send sizing survey to [john@battscan.ca](mailto:john@battscan.ca) or call 519-856-1380 For more information visit [www.FreshAireUV.com](http://www.FreshAireUV.com).

***Project Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Company Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Unit Number and Unit location\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Wholesaler Info \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

***Jobsite Contact\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Application (i.e. hospital, school, agriculture)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***

**\*\*PHOTOS REQUESTED IF AVAILABLE\*\***

1. **AHU TYPE: \_\_\_\_\_\_ *DX \_\_\_\_\_Chilled water \_\_\_\_\_Roof Top Package unit***
2. **AHU INFO: *MAKE \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Model # \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ CFM \_\_\_\_\_\_\_\_\_\_\_\_***
3. **COIL SIZE: *(Measured in \_\_\_\_ Inches \_\_\_\_Centimeters) \_\_\_\_\_\_\_\_Wide x \_\_\_\_\_\_\_ High Coil Depth \_\_\_\_\_\_\_\_\_\_***
4. **STACKED COILS? *\_\_\_\_\_\_\_* CENTER DRAIN PAN ? *\_\_\_\_\_\_\_\_\_ Coil Coating? YES NO***
5. **VOLTAGE: \_\_\_\_\_*120VAC \_\_\_\_\_208/230VAC \_\_\_\_\_277VAC \_\_\_\_\_ 460/480VAC***
6. **BELTS/ WIRES/RUBBER / FILTERS NEAR COIL? \_\_\_\_\_ *YES \_\_\_\_\_ NO***
7. **COIL / BLOWER DISTANCE: \_\_\_\_\_\_\_\_\_\_\_\_\_\_**
8. **COIL CONDITION:\_\_\_\_\_*CLEAN \_\_\_\_\_DIRTY Comments: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***
9. **INSTALL BY: \_\_\_\_\_\_*INHOUSE \_\_\_\_\_CONTRACTOR***
10. **CURRENTY USING UVC PRODUCTS? *YES NO Manufacturer: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_***
11. **INTERESTED IN: *\_\_\_\_\_\_ COIL CLEAN \_\_\_\_\_ ODOR CONTROL \_\_\_\_\_AIRBORNE DISINFECTION***
12. **IF INTERESTED IN AIRBORNE DISINFECTION, PLEASE PROVIDE:**

***DUCT SIZE: \_\_\_\_\_\_Wide x \_\_\_\_\_\_High DUCT Length: \_\_\_\_\_\_ DUCT MATERIAL: \_\_\_\_\_\_\_\_\_\_\_\_***

